|  |  |
| --- | --- |
| **Command** | **Description** |
| ip route 50.50.50.0/24 192.168.0.1 | Adds a static route to the device's configuration. |
| write | Saves the current configuration to the device. |